



**MTK Software upgrade tool operation guide**

Step 1: The driver installation instructions


Win7\_WinXP running



Next




Click Finish




Step 2: Open the Flash\_tool to upgrade


(1). Find the SP\_Flash\_Tool\_exe\_Windows\_v5.1512.00.000 Folder, enter, find the .exe file , run it




The tool UI as bellow



(2). Click **Scatter-loading**, Select MT6735\_Android\_scatter.txt file from the **full\_PL\_T2-4G\_9.88\_WJ\_EN\_1.6.91** Folder



(3). Select Download Only mode, and then click Download. as the picture. Wait for it finish.



(4). Connect the CAR DVR and the laptop with the USB data cable. Supply power for the car dvr (all the time during the processing). Then press the **R** button on the top of the DVR. When it finished, the UI as bellow picture.

